{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Generation","Demand","NTC"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Generation","index":0,"n_rows":309,"n_cols":5,"rows_kept":309,"cut":false,"hidden":false,"merged":[[181,1,192,2],[193,1,204,2]]}
[{"$nulls":4},"Harmonization"]
["Installed capacity [MW]","Nuclear",null,"DE",10793]
[null,null,null,"AT",0]
[null,null,null,"BE",5926]
[null,null,null,"CH",3333]
[null,null,null,"CZ",4040]
[null,null,null,"DK",0]
[null,null,null,"FR",63130]
[null,null,null,"LU",0]
[null,null,null,"NL",486]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",9714]
[null,"Lignite",null,"DE",20863]
[null,null,null,"AT",0]
[null,null,null,"BE",0]
[null,null,null,"CH",0]
[null,null,null,"CZ",7929]
[null,null,null,"DK",0]
[null,null,null,"FR",0]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",8576]
[null,null,null,"SE",0]
[null,"Hard Coal",null,"DE",26818]
[null,null,null,"AT",1171]
[null,null,null,"BE",0]
[null,null,null,"CH",0]
[null,null,null,"CZ",1200]
[null,null,null,"DK",4550]
[null,null,null,"FR",2997]
[null,null,null,"LU",0]
[null,null,null,"NL",4608]
[null,null,null,"NO",0]
[null,null,null,"PL",17906]
[null,null,null,"SE",225]
[null,"Natural Gas",null,"DE",24039.4]
[null,null,null,"AT",4820]
[null,null,null,"BE",6546]
[null,null,null,"CH",0]
[null,null,null,"CZ",1606]
[null,null,null,"DK",2431]
[null,null,null,"FR",11679]
[null,null,null,"LU",495]
[null,null,null,"NL",19297]
[null,null,null,"NO",445]
[null,null,null,"PL",1240]
[null,null,null,"SE",879]
[null,"Oil",null,"DE",2946]
[null,null,null,"AT",174]
[null,null,null,"BE",160]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",839]
[null,null,null,"FR",7130]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",332]
[null,null,null,"SE",3277]
[null,"Run of river",null,"DE",3856]
[null,null,null,"AT",4837.7]
[null,null,null,"BE",59]
[null,null,null,"CH",4844.8]
[null,null,null,"CZ",40.200000000000003]
[null,null,null,"DK",0]
[null,null,null,"FR",6051.5]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",14.4]
[null,null,null,"SE",1995]
[null,"Reservoir",null,"DE",202.8]
[null,null,null,"AT",5238.3999999999996]
[null,null,null,"BE",12.7]
[null,null,null,"CH",9186]
[null,null,null,"CZ",711.5]
[null,null,null,"DK",0]
[null,null,null,"FR",9043.6]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",31836.9]
[null,null,null,"PL",412.5]
[null,null,null,"SE",11645.8]
[null,"Bioenergy",null,"DE",6908]
[null,null,null,"AT",596]
[null,null,null,"BE",823]
[null,null,null,"CH",248]
[null,null,null,"CZ",850]
[null,null,null,"DK",1178]
[null,null,null,"FR",1046]
[null,null,null,"LU",11]
[null,null,null,"NL",486]
[null,null,null,"NO",2]
[null,null,null,"PL",933]
[null,null,null,"SE",2978]
[null,"Wind Onshore",null,"DE",45004]
[null,null,null,"AT",2489]
[null,null,null,"BE",1580]
[null,null,null,"CH",60]
[null,null,null,"CZ",277]
[null,null,null,"DK",3978]
[null,null,null,"FR",11762]
[null,null,null,"LU",120]
[null,null,null,"NL",3479]
[null,null,null,"NO",869]
[null,null,null,"PL",5697]
[null,null,null,"SE",6029]
[null,"Wind Offshore",null,"DE",4122]
[null,null,null,"AT",0]
[null,null,null,"BE",712]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",1271]
[null,null,null,"FR",0]
[null,null,null,"LU",0]
[null,null,null,"NL",638]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",0]
[null,"Solar",null,"DE",39791]
[null,null,null,"AT",732]
[null,null,null,"BE",3087]
[null,null,null,"CH",1061]
[null,null,null,"CZ",2027]
[null,null,null,"DK",851]
[null,null,null,"FR",6772]
[null,null,null,"LU",121]
[null,null,null,"NL",2039]
[null,null,null,"NO",0]
[null,null,null,"PL",186]
[null,null,null,"SE",0]
[null,"Geothermal",null,"DE",38]
[null,null,null,"AT",1]
[null,null,null,"BE",0]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",0]
[null,null,null,"FR",0]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",0]
[null,"Waste",null,"DE",1298]
[null,null,null,"AT",23]
[null,null,null,"BE",313]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",376]
[null,null,null,"FR",881]
[null,null,null,"LU",21]
[null,null,null,"NL",678]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",0]
[null,"Other conventional",null,"DE",3008]
[null,null,null,"AT",984]
[null,null,null,"BE",59]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",44]
[null,null,null,"FR",0]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",903]
[null,null,null,"SE",0]
[null,"Other renewable",null,"DE",508]
[null,null,null,"AT",0]
[null,null,null,"BE",0]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",0]
[null,null,null,"FR",1728]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",0]
["Pumped Hydro","Storage Capacity [MWh]",null,"DE",{"$f":"8*E194","v":50857.599999999999}]
[null,null,null,"AT",28714.400000000001]
[null,null,null,"BE",10464]
[null,null,null,"CH",35897.599999999999]
[null,null,null,"CZ",9380]
[null,null,null,"DK",0]
[null,null,null,"FR",42432]
[null,null,null,"LU",10328]
[null,null,null,"NL",0]
[null,null,null,"NO",10754.4]
[null,null,null,"PL",13640]
[null,null,null,"SE",736]
[null,"Generation Capacity [MW]",null,"DE",6357.2]
[null,null,null,"AT",3589.3]
[null,null,null,"BE",1308]
[null,null,null,"CH",4487.2]
[null,null,null,"CZ",1172.5]
[null,null,null,"DK",0]
[null,null,null,"FR",5304]
[null,null,null,"LU",1291]
[null,null,null,"NL",0]
[null,null,null,"NO",1344.3]
[null,null,null,"PL",1705]
[null,null,null,"SE",92]
["Fuel costs [€/MWh fuel]",null,null,"Nuclear",3.4369999999999998]
[null,null,null,"Lignite",2.9459999999999997]
[null,null,null,"Hard coal",9.3980358680057403]
[null,null,null,"Natural gas",15.4435665643125]
[null,null,null,"Light Oil",22.3797465986395]
[null,null,null,"Heavy Oil",22.379746598639453]
[null,null,null,"Biomass",0]
["CO2 cost [€/t CO2]",null,null,"CO2",5.1653199999999995]
["Annual capcity factors","Wind Onshore",null,"DE",0.16700000000000001]
[null,null,null,"AT",0.23799999999999999]
[null,null,null,"BE",0.19500000000000001]
[null,null,null,"CH",0.19]
[null,null,null,"CZ",0.20499999999999999]
[null,null,null,"DK",0.23200000000000001]
[null,null,null,"FR",0.2]
[null,null,null,"LU",9.5000000000000001E-2]
[null,null,null,"NL",0.19]
[null,null,null,"NO",0.27500000000000002]
[null,null,null,"PL",0.24399999999999999]
[null,null,null,"SE",0.28999999999999998]
[null,"Wind Offshore",null,"DE",0.33400000000000002]
[null,null,null,"AT",0]
[null,null,null,"BE",0.38400000000000001]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",0.42099999999999999]
[null,null,null,"FR",0]
[null,null,null,"LU",0]
[null,null,null,"NL",0.35699999999999998]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",0]
[null,"Solar",null,"DE",0.1]
[null,null,null,"AT",0.122]
[null,null,null,"BE",0.107]
[null,null,null,"CH",5.3999999999999999E-2]
[null,null,null,"CZ",0.11799999999999999]
[null,null,null,"DK",9.4E-2]
[null,null,null,"FR",0.14099999999999999]
[null,null,null,"LU",9.4E-2]
[null,null,null,"NL",8.4000000000000005E-2]
[null,null,null,"NO",0]
[null,null,null,"PL",6.0999999999999999E-2]
[null,null,null,"SE",5.6000000000000001E-2]
[null,"Bioenergy",null,"DE",0.67073312217929526]
[null,null,null,"AT",0]
[null,null,null,"BE",0.47031275244728626]
[null,null,null,"CH",0.18361830894882192]
[null,null,null,"CZ",0.57591342547948143]
[null,null,null,"DK",0.33824425332677721]
[null,null,null,"FR",0.45711479589171344]
[null,null,null,"LU",1]
[null,null,null,"NL",0.8198595276109949]
[null,null,null,"NO",0]
[null,null,null,"PL",0.87853390262330222]
[null,null,null,"SE",0.34405311079060652]
[null,"Waste",null,"DE",0.8770674233302741]
[null,null,null,"AT",0]
[null,null,null,"BE",0.87292026746276996]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",0.42388481959462077]
[null,null,null,"FR",0.55564859438996506]
[null,null,null,"LU",0.54211119784890272]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",0]
[null,"Other renewable",null,"DE",0.33615162858741016]
[null,null,null,"AT",0]
[null,null,null,"BE",0]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",0]
[null,null,null,"FR",0]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",0]
[null,"Reservoir",null,"DE",0.11329404707759036]
[null,null,null,"AT",0.18940662691918755]
[null,null,null,"BE",9.5739821638453015E-2]
[null,null,null,"CH",0.32513401094977035]
[null,null,null,"CZ",0.14784850850424622]
[null,null,null,"DK",0]
[null,null,null,"FR",1]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0.53060540878284712]
[null,null,null,"PL",7.0165393866421927E-2]
[null,null,null,"SE",0.43050006888001102]
[null,"Run of river",null,"DE",0.60135832329687033]
[null,null,null,"AT",0.50869600744811383]
[null,null,null,"BE",0.2799426677416465]
[null,null,null,"CH",0.23976143563832469]
[null,null,null,"CZ",0.23859385055026558]
[null,null,null,"DK",0]
[null,null,null,"FR",0.17571755914317827]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",0.3849775173129889]
[null,null,null,"SE",0]

{"sheet":"Demand","index":1,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Yearly total electricity demand [TWh]","Harmonization"]
["AT",67.599999999999994]
["BE",87]
["CH",60.2]
["CZ",63.9]
["DK",34.1]
["FR",484.7]
["LU",6.5]
["NL",115.9]
["NO",131.80000000000001]
["PL",153.30000000000001]
["SE",140.6]
["DE",556.1]

{"sheet":"NTC","index":2,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[[0,1,0,4]]}
["MW","Harmonization",null,null,null,"Comments"]
["Germany-Neighbors"]
["DE-AT","DE-AT",9000,"AT-DE",9000,"Common market zone in 2017"]
["DE-BE","DE-BE",0,"BE-DE",0]
["DE-CH","DE-CH",1586,"CH-DE",4000]
["DE-CZ","DE-CZ",1500,"CZ-DE",1586]
["DE-DK","DE-DK",2100,"DK-DE",2165]
["DE-FR","DE-FR",2300,"FR-DE",1800]
["DE-LU","DE-LU",2300,"LU-DE",2300,"Common market zone in 2017"]
["DE-NL","DE-NL",4250,"NL-DE",2881]
["DE-NO","DE-NO",0,"NO-DE",0]
["DE-PL","DE-PL",500,"PL-DE",2500]
["DE-SE","DE-SE",615,"SE-DE",615]
["Neighbors-Neighbors"]
["BE-FR","BE-FR",1800,"FR-BE",3300]
["BE-LU","BE-LU",680,"LU-BE",180]
["BE-NL","BE-NL",2400,"NL-BE",1400]
["FR-LU","FR-LU",380,"LU-FR",0]
["FR-CH","FR-CH",3150,"CH-FR",1300]
["CH-AT","CH-AT",1200,"AT-CH",1200]
["CZ-AT","CZ-AT",800,"AT-CZ",900]
["CZ-PL","CZ-PL",600,"PL-CZ",800]
["SE-DK","SE-DK",1300,"DK-SE",1700]
["SE-NO","SE-NO",3995,"NO-SE",3695]
["SE-PL","SE-PL",600,"PL-SE",600]
["NO-NL","NO-NL",700,"NL-NO",700]
["NO-DK","NO-DK",1640,"DK-NO",1640]