{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Generation","Demand","NTC"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Generation","index":0,"n_rows":309,"n_cols":5,"rows_kept":309,"cut":false,"hidden":false,"merged":[[181,1,192,2],[193,1,204,2]]}
[{"$nulls":4},"Harmonization"]
["Installed capacity [MW]","Nuclear",null,"DE",0]
[null,null,null,"AT",0]
[null,null,null,"BE",0]
[null,null,null,"CH",1190]
[null,null,null,"CZ",4055]
[null,null,null,"DK",0]
[null,null,null,"FR",37640]
[null,null,null,"LU",0]
[null,null,null,"NL",486]
[null,null,null,"NO",0]
[null,null,null,"PL",3000]
[null,null,null,"SE",6852]
[null,"Lignite",null,"DE",9300]
[null,null,null,"AT",0]
[null,null,null,"BE",0]
[null,null,null,"CH",0]
[null,null,null,"CZ",4760]
[null,null,null,"DK",0]
[null,null,null,"FR",0]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",7405]
[null,null,null,"SE",0]
[null,"Hard Coal",null,"DE",9800]
[null,null,null,"AT",0]
[null,null,null,"BE",0]
[null,null,null,"CH",0]
[null,null,null,"CZ",251]
[null,null,null,"DK",410]
[null,null,null,"FR",0]
[null,null,null,"LU",0]
[null,null,null,"NL",4608]
[null,null,null,"NO",0]
[null,null,null,"PL",13771]
[null,null,null,"SE",80]
[null,"Natural Gas",null,"DE",29800]
[null,null,null,"AT",4164]
[null,null,null,"BE",6352]
[null,null,null,"CH",0]
[null,null,null,"CZ",1379]
[null,null,null,"DK",430]
[null,null,null,"FR",11496]
[null,null,null,"LU",0]
[null,null,null,"NL",7592.8]
[null,null,null,"NO",435]
[null,null,null,"PL",5741]
[null,null,null,"SE",0]
[null,"Oil",null,"DE",900]
[null,null,null,"AT",174]
[null,null,null,"BE",0]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",817]
[null,null,null,"FR",1479]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",0]
[null,"Run of river",null,"DE",4831.8]
[null,null,null,"AT",4671.89977]
[null,null,null,"BE",117]
[null,null,null,"CH",4139]
[null,null,null,"CZ",365]
[null,null,null,"DK",6.6082000000000001]
[null,null,null,"FR",13797]
[null,null,null,"LU",34]
[null,null,null,"NL",38]
[null,null,null,"NO",0]
[null,null,null,"PL",1033]
[null,null,null,"SE",0]
[null,"Reservoir",null,"DE",268.2]
[null,null,null,"AT",10842.850999999901]
[null,null,null,"BE",1308]
[null,null,null,"CH",13580]
[null,null,null,"CZ",1050]
[null,null,null,"DK",0]
[null,null,null,"FR",13697]
[null,null,null,"LU",1310]
[null,null,null,"NL",0]
[null,null,null,"NO",35816.9]
[null,null,null,"PL",1413]
[null,null,null,"SE",16184]
[null,"Bioenergy",null,"DE",6000]
[null,null,null,"AT",599]
[null,null,null,"BE",206]
[null,null,null,"CH",1197]
[null,null,null,"CZ",1063]
[null,null,null,"DK",671]
[null,null,null,"FR",2558]
[null,null,null,"LU",54]
[null,null,null,"NL",540]
[null,null,null,"NO",76]
[null,null,null,"PL",1414]
[null,null,null,"SE",4185]
[null,"Wind Onshore",null,"DE",81500]
[null,null,null,"AT",5000]
[null,null,null,"BE",3298]
[null,null,null,"CH",370]
[null,null,null,"CZ",950]
[null,null,null,"DK",5596]
[null,null,null,"FR",36336]
[null,null,null,"LU",200]
[null,null,null,"NL",6722.98]
[null,null,null,"NO",3330.3]
[null,null,null,"PL",9200]
[null,null,null,"SE",10780]
[null,"Wind Offshore",null,"DE",17000]
[null,null,null,"AT",0]
[null,null,null,"BE",2310]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",2905]
[null,null,null,"FR",7000]
[null,null,null,"LU",0]
[null,null,null,"NL",11500]
[null,null,null,"NO",0]
[null,null,null,"PL",2250]
[null,null,null,"SE",190]
[null,"Solar",null,"DE",91300]
[null,null,null,"AT",4500]
[null,null,null,"BE",5050.5]
[null,null,null,"CH",5600]
[null,null,null,"CZ",3540]
[null,null,null,"DK",2939]
[null,null,null,"FR",31565]
[null,null,null,"LU",200]
[null,null,null,"NL",11439]
[null,null,null,"NO",400]
[null,null,null,"PL",2430]
[null,null,null,"SE",1740]
[null,"Geothermal",null,"DE"]
[null,null,null,"AT"]
[null,null,null,"BE"]
[null,null,null,"CH"]
[null,null,null,"CZ"]
[null,null,null,"DK"]
[null,null,null,"FR"]
[null,null,null,"LU"]
[null,null,null,"NL"]
[null,null,null,"NO"]
[null,null,null,"PL"]
[null,null,null,"SE"]
[null,"Waste",null,"DE",1700]
[null,null,null,"AT",144]
[null,null,null,"BE",361]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",363]
[null,null,null,"FR",0]
[null,null,null,"LU",21]
[null,null,null,"NL",674]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",0]
[null,"Other conventional",null,"DE",300]
[null,null,null,"AT",984]
[null,null,null,"BE",1157]
[null,null,null,"CH",985]
[null,null,null,"CZ",1505]
[null,null,null,"DK",99.1]
[null,null,null,"FR",0]
[null,null,null,"LU",90]
[null,null,null,"NL",3539]
[null,null,null,"NO",0]
[null,null,null,"PL",7276]
[null,null,null,"SE",390]
[null,"Other renewable",null,"DE",600]
[null,null,null,"AT",620]
[null,null,null,"BE",658]
[null,null,null,"CH",1300]
[null,null,null,"CZ",1167]
[null,null,null,"DK",700.4]
[null,null,null,"FR",3638]
[null,null,null,"LU",51.3]
[null,null,null,"NL",507]
[null,null,null,"NO",76.302999999999997]
[null,null,null,"PL",1756]
[null,null,null,"SE",4203]
["Pumped Hydro","Storage Capacity [MWh]",null,"DE",{"$f":"E194*8","v":88000}]
[null,null,null,"AT",{"$f":"E195*8","v":48442.663999999997}]
[null,null,null,"BE",9200]
[null,null,null,"CH",36744]
[null,null,null,"CZ",8000]
[null,null,null,"DK",0]
[null,null,null,"FR",44000]
[null,null,null,"LU",8208]
[null,null,null,"NL",0]
[null,null,null,"NO",8917.6640000000007]
[null,null,null,"PL",11904]
[null,null,null,"SE",0]
[null,"Generation Capacity [MW]",null,"DE",11000]
[null,null,null,"AT",6055.3329999999996]
[null,null,null,"BE",1150]
[null,null,null,"CH",4593]
[null,null,null,"CZ",1000]
[null,null,null,"DK",0]
[null,null,null,"FR",5500]
[null,null,null,"LU",1026]
[null,null,null,"NL",0]
[null,null,null,"NO",1114.7080000000001]
[null,null,null,"PL",1488]
[null,null,null,"SE",0]
["Fuel costs [€/MWh fuel]",null,null,"Nuclear",3.4]
[null,null,null,"Lignite",5.5]
[null,null,null,"Hard coal",12.6]
[null,null,null,"Natural gas",25.9]
[null,null,null,"Light Oil",60]
[null,null,null,"Heavy Oil",60]
[null,null,null,"Biomass",32.5]
["CO2 cost [€/t CO2]",null,null,"CO2",26.8]
["Annual capcity factors","Wind Onshore",null,"DE",{"$f":"173.8/(81.5*8.76)","v":0.24343782390677091}]
[null,null,null,"AT",0.183]
[null,null,null,"BE",0.19500000000000001]
[null,null,null,"CH",0.20799999999999999]
[null,null,null,"CZ",0.23799999999999999]
[null,null,null,"DK",0.23200000000000001]
[null,null,null,"FR",0.25800000000000001]
[null,null,null,"LU",0.22700000000000001]
[null,null,null,"NL",0.19]
[null,null,null,"NO",0.313]
[null,null,null,"PL",0.26100000000000001]
[null,null,null,"SE",0.28999999999999998]
[null,"Wind Offshore",null,"DE",{"$f":"73.8/(17*8.76)","v":0.49556809024979859}]
[null,null,null,"AT",0]
[null,null,null,"BE",0.38400000000000001]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",0.42099999999999999]
[null,null,null,"FR",0]
[null,null,null,"LU",0]
[null,null,null,"NL",0.35699999999999998]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",0]
[null,"Solar",null,"DE",{"$f":"86.8/(91.3*8.76)","v":0.10852876012143217}]
[null,null,null,"AT",0.13400000000000001]
[null,null,null,"BE",0.34300000000000003]
[null,null,null,"CH",0.112]
[null,null,null,"CZ",0.122]
[null,null,null,"DK",0.12]
[null,null,null,"FR",0.13300000000000001]
[null,null,null,"LU",0.106]
[null,null,null,"NL",9.9000000000000005E-2]
[null,null,null,"NO",0.104]
[null,null,null,"PL",0.1]
[null,null,null,"SE",0.108]
[null,"Bioenergy",null,"DE",0.64]
[null,null,null,"AT",0.63700000000000001]
[null,null,null,"BE",0.70899999999999996]
[null,null,null,"CH",0.42699999999999999]
[null,null,null,"CZ",0.441]
[null,null,null,"DK",0.58199999999999996]
[null,null,null,"FR",0.47799999999999998]
[null,null,null,"LU",0.58199999999999996]
[null,null,null,"NL",0.8198595276109949]
[null,null,null,"NO",0.86499999999999999]
[null,null,null,"PL",0.48499999999999999]
[null,null,null,"SE",0.44]
[null,"Waste",null,"DE",0.8770674233302741]
[null,null,null,"AT",0]
[null,null,null,"BE",0.87292026746276996]
[null,null,null,"CH",0]
[null,null,null,"CZ",0]
[null,null,null,"DK",0.42388481959462077]
[null,null,null,"FR",0.55564859438996506]
[null,null,null,"LU",0.54211119784890272]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",0]
[null,null,null,"SE",0]
[null,"Other renewable",null,"DE",0]
[null,null,null,"AT",0.63700000000000001]
[null,null,null,"BE",0.70899999999999996]
[null,null,null,"CH",0.42699999999999999]
[null,null,null,"CZ",0.441]
[null,null,null,"DK",0.58199999999999996]
[null,null,null,"FR",0.47799999999999998]
[null,null,null,"LU",0.58199999999999996]
[null,null,null,"NL",0.8198595276109949]
[null,null,null,"NO",0.86499999999999999]
[null,null,null,"PL",0.48499999999999999]
[null,null,null,"SE",0.44]
[null,"Reservoir",null,"DE",0.11329404707759036]
[null,null,null,"AT",0.18940662691918755]
[null,null,null,"BE",9.5739821638453015E-2]
[null,null,null,"CH",0.32513401094977035]
[null,null,null,"CZ",0.14784850850424622]
[null,null,null,"DK",0]
[null,null,null,"FR",1]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0.53060540878284712]
[null,null,null,"PL",7.0165393866421927E-2]
[null,null,null,"SE",0.43050006888001102]
[null,"Run of river",null,"DE",0.60135832329687033]
[null,null,null,"AT",0.50869600744811383]
[null,null,null,"BE",0.2799426677416465]
[null,null,null,"CH",0.23976143563832469]
[null,null,null,"CZ",0.23859385055026558]
[null,null,null,"DK",0]
[null,null,null,"FR",0.17571755914317827]
[null,null,null,"LU",0]
[null,null,null,"NL",0]
[null,null,null,"NO",0]
[null,null,null,"PL",0.3849775173129889]
[null,null,null,"SE",0]

{"sheet":"Demand","index":1,"n_rows":13,"n_cols":2,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
["Yearly total electricity demand [TWh]","Harmonization"]
["AT",76.3]
["BE",88.4]
["CH",58.3]
["CZ",70.7]
["DK",46.6]
["FR",464.9]
["LU",11]
["NL",118.1]
["NO",148.19999999999999]
["PL",206.4]
["SE",141.30000000000001]
["DE",546.4]

{"sheet":"NTC","index":2,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[[0,1,0,4]]}
["MW","Harmonization",null,null,null,"Comments"]
["Germany-Neighbors"]
["DE-AT","DE-AT",5400,"AT-DE",5400,"Common market zone in 2017"]
["DE-BE","DE-BE",1000,"BE-DE",1000]
["DE-CH","DE-CH",2700,"CH-DE",4600]
["DE-CZ","DE-CZ",1500,"CZ-DE",2100]
["DE-DK","DE-DK",4100,"DK-DE",{"$f":"585+3500","v":4085}]
["DE-FR","DE-FR",3000,"FR-DE",3000]
["DE-LU","DE-LU",2300,"LU-DE",2300,"Common market zone in 2017"]
["DE-NL","DE-NL",5000,"NL-DE",5000]
["DE-NO","DE-NO",1400,"NO-DE",1400]
["DE-PL","DE-PL",2000,"PL-DE",3000]
["DE-SE","DE-SE",615,"SE-DE",615]
["Neighbors-Neighbors"]
["BE-FR","BE-FR",2800,"FR-BE",4300]
[" BE-LU","BE-LU",680,"LU-BE",100]
["BE-NL","BE-NL",2400,"NL-BE",2400]
["FR-LU","FR-LU",380,"LU-FR",0]
["FR-CH","FR-CH",3700,"CH-FR",1300]
["CH-AT","CH-AT",1200,"AT-CH",1200]
["CZ-AT","CZ-AT",900,"AT-CZ",900]
["CZ-PL","CZ-PL",600,"PL-CZ",800]
["SE-DK","SE-DK",1295,"DK-SE",2440]
["SE-NO","SE-NO",3995,"NO-SE",3695]
["SE-PL","SE-PL",600,"PL-SE",600]
["NO-NL","NO-NL",700,"NL-NO",700]
["NO-DK","NO-DK",1600,"DK-NO",1640]
["NL-DK","NL-DK",700,"DK-NL",700]